{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":136,"n_cols":6,"rows_kept":136,"flags":["formulas_cached_only"]}
["Type","Unit","k","b","Digit","Remark"]
["length","in",1,0,null,"inch"]
["length","m",39.37007874015748,0,null,"meter"]
["length","cm",0.3937007874015748,0,null,"centimeter"]
["length","mm",0.03937007874015748,0,null,"milimeter"]
["length","km",39370.078740157485,0,null,"kilometer"]
["length","ft",12,0,null,"feet"]
["length","mi",63346.45669291339,0,null,"mile"]
["length","yd",35.98728346456693,0,null,"yard"]
["length","nmile",72913.38582677166,0,null,"nautical mile"]
["length","nm",{"v":3.9370078740157486e-08,"d":"3.94E-08"},0,null,"nanometer "]
["length","rad",7.828307086614173,0,null,"rad"]
["square","m^2",1,0,null,"square meter"]
["square","km^2",1000000,0,null,"square kilometer"]
["square","in^2",0.0006452,0,null,"square inch"]
["square","cm^2",0.0001,0,null,"square centimeter"]
["square","acre",4047,0,null,"acre"]
["square","mile^2",2588881,0,null,"square mile"]
["square","ft^2",0.093,0,null,"square feet"]
["square","ha",10000,0,null,"hectare"]
["square","yd^2",0.8361,0,null,"square yard"]
["square","rad2",0.0395368604,0,null,"square rad"]
["volume","m^3",1,0,null,"cubic meter"]
["volume","ml",1e-06,0,null,"milliliter"]
["volume","L",0.001,0,null,"liter"]
["volume","in^3",1.639e-05,0,null,"cubic inch"]
["volume","cm^3",1e-06,0,null,"cubic centimeter"]
["volume","pt",0.000473,0,null,"pint"]
["volume","gal(US)",0.003785,0,null,"gallon(US)"]
["volume","bbl",0.159,0,null,"barrel"]
["volume","bcf",2831700,0,null,"billion cubic feet"]
["volume","tcf",28317000000,0,null,"trillions of cubic feet"]
["volume","mmcf",28317,0,null,"million cubic feet"]
["volume","mcf",28.317,0,null,"thousand cubic feet"]
["volume","ft^3",0.0283,0,null,"cubic feet"]
["volume","gal(UK)",0.004546,0,null,"gallon(UK)"]
["volume","gi",0.000118,0,null,"gill"]
["volume","qt",0.000946,0,null,"quart"]
["volume","cc",1e-06,0,null,"cubic centimeter"]
["volume","acre.ft",1234,0,null,"acres*feet"]
["weight","kg",1,0,null,"killogrammeter"]
["weight","ton",1000,0,null,"ton"]
["weight","lton",1016,0,null,"long ton "]
["weight","lb",0.454,0,null,"pound"]
["weight","oz",0.02835,0,null,"ounce"]
["weight","ston",907,0,null,"short ton"]
["weight","g",0.001,0,null,"grammeter"]
["density","g/cm^3",1,0,null,"grammeter per cubic centimeter"]
["density","kg/m^3",0.001,0,null,"killogrammeter per cubic meter"]
["density","lb/ft^3",0.01602,0,null,"pound per cubic feet"]
["density","lb/gal(US)",0.119826,0,null,"pound per cubic gallen"]
["density","lb/gal(UK)",0.09976,0,null,"pound per cubic gallen"]
["density","lb/bbl",0.002853,0,null,"pound per barrle"]
["density","g/cc",1,0,null,"grammeter per cubic centimeter"]
["density","g/cf",3.53147e-05,0,null,"grammeter per cubic feet"]
["density","g/ft^3",3.53147e-05,0,null,"grammeter per cubic feet"]
["viscosity act","m^2/s",1,0,null,"square meter per second"]
["viscosity act","cm^2/s",0.0001,0,null,"square cenmeter per second"]
["viscosity act","ft^2/s",0.092903,0,null,"square feet per second"]
["viscosity act","St",0.0001,0,null,"sthene"]
["viscosity act","cSt",1e-06,0,null,"centisthene"]
["viscosity act","mm^2/s",1e-06,0,null,"square millimeter per second"]
["viscosity","Pa.s",1,0,null,"pascal second "]
["viscosity","mPa·s",0.001,0,null,"pascal second "]
["viscosity","P",0.1,0,null,"poise"]
["viscosity","cP",0.001,0,null,"centipoise"]
["viscosity","bf.s/ft^2",47.8803,0,null,"pound centisecond per cubic feet"]
["viscosity","kgf.s/m^3",9.80665,0,null,"killogrammeter centisecond per cubic meter"]
["strength","N",1,0,null,"newton"]
["strength","lbf",4.4444444444,0,null,"pound force"]
["strength","kgf",9.81,0,null,"kilogram force"]
["strength","dyn",1e-05,0,null,"dyne"]
["temperature","deg",1,0,null,"centigrade"]
["temperature","K",1,273.15,null,"kelvin"]
["temperature","F",1.8,null,null,"fahrenheit"]
["temperature"," ℃",1,0,null,"centigrade"]
["pressure","Pa",1,0,null,"pascal  "]
["pressure","MPa",1000000,0,null,"pascal  "]
["pressure","KPa",1000,0,null,"pascal  "]
["pressure","bar",100000,0,null,"bar "]
["pressure","Torr",133.322,0,null,"torr"]
["pressure","dyn/cm^2",0.1,0,null,"dyne per square centimeter"]
["pressure","mmHg",133.322,0]
["pressure","mmH2O",9.80665,0]
["pressure","at",98066.5,0,null,"effective atmosphere"]
["pressure","psi",6896.5517241379,0,null,"pound per cubic inch "]
["pressure","atm",101325,0,null,"standard atomsphere pressure"]
["pressure","kgf/cm^2",98079.6586059744,0,null,"kilometer per square centimeter "]
["themal power","J",1,0,null,"joule"]
["themal power","cal",4.1868,0,null,"calorie"]
["themal power","kgf.m",9.80665,0,null,"kilogram force meter"]
["themal power","Btu",1055.06,0,null,"britishthermalunit"]
["themal power","kW.h",3600000,0,null,"kilowatt hour"]
["themal power","ft.lbf",1.35582,0,null,"feet pound force"]
["themal power","hp.h(US)",2647790,0,null,"US horsepower hour"]
["themal power","Hp.h(UK)",2684520,0,null,"UK horsepower hour"]
["themal power","kg.m",9.8000784006,0,null,"killogrammeter"]
["themal power","kcal",4185.8518208455,0,null,"kilocalorie"]
["themal power","BTU",1054.8523206751,0,null,"british thermal"]
["power","W",1,0,null,"watt"]
["power","Btu/h",0.293071,0,null,"britishthermalunit per hour"]
["power","kgf.m/s",9.80665,0,null,"kilogramer force mile per second"]
["power","cal/s",4.1868,0,null,"calorie per second"]
["power","hp",735.499,0,null,"horsepower "]
["velocity","m/s",1,0,null,"mile per second"]
["velocity","mile/h",0.44704,0,null,"mile per hour"]
["velocity","ft/s",0.3048,0,null,"feet per second"]
["slowness","us/m",1,0,null,"microsecond per mile "]
["slowness","us/ft",3.28084,0,null,"microsecond per feet"]
["permeability","D",1,0,null,"darcy"]
["permeability","mD",0.001,0,null,"millidarcy"]
["permeability","cm^-2",98100000,0,null,"per square centimeter"]
["geothermalgradient","deg/m",1,0,null,"centigrade per meter"]
["geothermalgradient","F/in",1.8,0,null,"kelvin per inch"]
["geothermalgradient","deg/km",0.099,0,null,"centigrade per kilometer"]
["geothermalgradient","F/mile",0.0344827586,0,null,"kelvin per mile "]
["geothermalgradient","F/ft",181.8181818182,0,null,"kelvin per feet"]
["production","m^3/d",1,0,null,"cubic meter per day"]
["production","tcf/d",0.02832,0,null,"trillions of cubic feet per day "]
["production","m^3/a",0.0027400706,0,null,"cubic meter per year"]
["production","bcf/d",0.02832,0,null,"billion cubic feet per day"]
["production","mmcf/d",28320,0,null,"million cubic feet per day"]
["production","mcf/d",28.32,0,null,"thousand cubic feet per day"]
["time ","us",1,0,null,"microsecond"]
["time ","ms",1000,0,null,"millisecond"]
["time ","s",1000000,0,null,"second"]
["voltage","mv",1,0,null,"millivoltage"]
["voltage","v",1000,0,null,"voltage"]
["radioactivity","gAPI",1,0,null,"generous American petroleum institude"]
["radioactivity","API",1,0,null,"American petroleum institude"]
["percent","%",1,0,null,"percent"]
["percent","pu",1,0,null,"porosity unit"]
["percent","m3/m3",100,0,null,"cubic meter per cubic meter"]
["percent","v/v",100,0,null,"volume per volume"]
["percent","dec",100,0,null,"Decimal"]
["Compressibility","1/Mpa",1,0,null,"Compressibility"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}